*Apr  8 15:11:55.604: csim: called number = 640123456789, loop count = 1 ping count = 0

*Apr  8 15:11:55.604: csimSetupPeer peer type(2), destPat(640123456789), matched(2), target()
*Apr  8 15:11:55.604: //-1/xxxxxxxxxxxx/CCAPI/ccCallSetupRequest:
   Destination=, Calling IE Present=FALSE, Mode=0,
   Outgoing Dial-peer=300, Params=0x6398E770, Progress Indication=NULL(0)
*Apr  8 15:11:55.604: //-1/xxxxxxxxxxxx/CCAPI/ccCheckClipClir:
   In: Calling Number=(TON=Unknown, NPI=Unknown, Screening=Not Screened, Presentation=Allowed)
*Apr  8 15:11:55.604: //-1/xxxxxxxxxxxx/CCAPI/ccCheckClipClir:
   Out: Calling Number=(TON=Unknown, NPI=Unknown, Screening=Not Screened, Presentation=Allowed)
*Apr  8 15:11:55.604: //-1/xxxxxxxxxxxx/CCAPI/ccCallSetupRequest:
   Destination Pattern=64T, Called Number=640123456789, Digit Strip=FALSE
*Apr  8 15:11:55.604: //-1/xxxxxxxxxxxx/CCAPI/ccCallSetupRequest:
   Calling Number=(TON=Unknown, NPI=Unknown, Screening=Not Screened, Presentation=Allowed),
   Called Number=640123456789(TON=Unknown, NPI=Unknown),
   Redirect Number=, Display Info=
   Account Number=, Final Destination Flag=FALSE,
   Guid=7C216977-9F95-11E2-8094-B73EFBDBDE30, Outgoing Dial-peer=300
*Apr  8 15:11:55.604: //-1/xxxxxxxxxxxx/CCAPI/cc_api_display_ie_subfields:
   ccCallSetupRequest:
   cisco-username=
   ----- ccCallInfo IE subfields -----
   cisco-ani=
   cisco-anitype=0
   cisco-aniplan=0
   cisco-anipi=0
   cisco-anisi=0
   dest=640123456789
   cisco-desttype=0
   cisco-destplan=0
   cisco-rdie=FFFFFFFF
   cisco-rdn=
   cisco-rdntype=-1
   cisco-rdnplan=-1
   cisco-rdnpi=-1
   cisco-rdnsi=-1
   cisco-redirectreason=-1   fwd_final_type =0
   final_redirectNumber =
   hunt_group_timeout =0

*Apr  8 15:11:55.608: //-1/xxxxxxxxxxxx/CCAPI/ccIFCallSetupRequestPrivate:
   Interface=0x65C57F24, Interface Type=1, Destination=, Mode=0x0,
   Call Params(Calling Number=,(Calling Name=)(TON=Unknown, NPI=Unknown, Screening=Not Screened, Presentation=Allowed),
   Called Number=640123456789(TON=Unknown, NPI=Unknown), Calling Translated=FALSE,
   Subscriber Type Str=, FinalDestinationFlag=FALSE, Outgoing Dial-peer=300, Call Count On=FALSE,
   Source Trkgrp Route Label=, Target Trkgrp Route Label=, tg_label_flag=0, Application Call Id=)
*Apr  8 15:11:55.608: //-1/xxxxxxxxxxxx/CCAPI/cc_get_feature_vsa:
   
*Apr  8 15:11:55.608: :cc_get_feature_vsa malloc success
*Apr  8 15:11:55.608: //-1/xxxxxxxxxxxx/CCAPI/cc_get_feature_vsa:
   
*Apr  8 15:11:55.608:  cc_get_feature_vsa count is 1
*Apr  8 15:11:55.608: //-1/xxxxxxxxxxxx/CCAPI/cc_get_feature_vsa:
   
*Apr  8 15:11:55.608: :FEATURE_VSA attributes are: feature_name:0,feature_time:1709500040,feature_id:36
*Apr  8 15:11:55.608: //33/7C2169778094/CCAPI/ccIFCallSetupRequestPrivate:
   SPI Call Setup Request Is Success; Interface Type=1, FlowMode=1
*Apr  8 15:11:55.608: //33/7C2169778094/CCAPI/ccCallSetContext:
   Context=0x66BCA144
*Apr  8 15:11:55.616: //-1/7C2169778094/CCAPI/cc_api_display_ie_subfields:
   cc_api_call_setup_ind_common:
   cisco-username=114.23.6.203
   ----- ccCallInfo IE subfields -----
   cisco-ani=
   cisco-anitype=0
   cisco-aniplan=0
   cisco-anipi=0
   cisco-anisi=0
   dest=00640123456789
   cisco-desttype=0
   cisco-destplan=0
   cisco-rdie=FFFFFFFF
   cisco-rdn=
   cisco-rdntype=-1
   cisco-rdnplan=-1
   cisco-rdnpi=-1
   cisco-rdnsi=-1
   cisco-redirectreason=-1   fwd_final_type =0
   final_redirectNumber =
   hunt_group_timeout =0

*Apr  8 15:11:55.616: //-1/7C2169778094/CCAPI/cc_api_call_setup_ind_common:
   Interface=0x65C57F24, Call Info(
   Calling Number=,(Calling Name=)(TON=Unknown, NPI=Unknown, Screening=Not Screened, Presentation=Allowed),
   Called Number=00640123456789(TON=Unknown, NPI=Unknown),
   Calling Translated=FALSE, Subscriber Type Str=Unknown, FinalDestinationFlag=TRUE,
   Incoming Dial-peer=100, Progress Indication=NULL(0), Calling IE Present=FALSE,
   Source Trkgrp Route Label=, Target Trkgrp Route Label=, CLID Transparent=FALSE), Call Id=34
*Apr  8 15:11:55.620: //-1/7C2169778094/CCAPI/ccCheckClipClir:
   In: Calling Number=(TON=Unknown, NPI=Unknown, Screening=Not Screened, Presentation=Allowed)
*Apr  8 15:11:55.620: //-1/7C2169778094/CCAPI/ccCheckClipClir:
   Out: Calling Number=(TON=Unknown, NPI=Unknown, Screening=Not Screened, Presentation=Allowed)
*Apr  8 15:11:55.620: //-1/xxxxxxxxxxxx/CCAPI/cc_get_feature_vsa:
   
*Apr  8 15:11:55.620: :cc_get_feature_vsa malloc success
*Apr  8 15:11:55.620: //-1/xxxxxxxxxxxx/CCAPI/cc_get_feature_vsa:
   
*Apr  8 15:11:55.620:  cc_get_feature_vsa count is 2
*Apr  8 15:11:55.620: //-1/xxxxxxxxxxxx/CCAPI/cc_get_feature_vsa:
   
*Apr  8 15:11:55.620: :FEATURE_VSA attributes are: feature_name:0,feature_time:1709500472,feature_id:37
*Apr  8 15:11:55.620: //34/7C2169778094/CCAPI/cc_api_call_setup_ind_common:
   Set Up Event Sent;
   Call Info(Calling Number=(TON=Unknown, NPI=Unknown, Screening=Not Screened, Presentation=Allowed),
   Called Number=00640123456789(TON=Unknown, NPI=Unknown))
*Apr  8 15:11:55.620: //34/7C2169778094/CCAPI/cc_process_call_setup_ind:
   Event=0x65E5D2F0
*Apr  8 15:11:55.620: //34/7C2169778094/CCAPI/ccCallSetContext:
   Context=0x66D4A830
*Apr  8 15:11:55.620: //34/7C2169778094/CCAPI/cc_process_call_setup_ind:
   >>>>CCAPI handed cid 34 with tag 100 to app "_ManagedAppProcess_voy"
*Apr  8 15:11:55.624: //-1/xxxxxxxxxxxx/CCAPI/ccCallSetupRequest:
   Destination=, Calling IE Present=TRUE, Mode=0,
   Outgoing Dial-peer=10, Params=0x66D4B6F8, Progress Indication=NULL(0)
*Apr  8 15:11:55.624: //-1/xxxxxxxxxxxx/CCAPI/ccCheckClipClir:
   In: Calling Number=1212121212(TON=National, NPI=ISDN, Screening=Not Screened, Presentation=Allowed)
*Apr  8 15:11:55.624: //-1/xxxxxxxxxxxx/CCAPI/ccCheckClipClir:
   Out: Calling Number=1212121212(TON=National, NPI=ISDN, Screening=Not Screened, Presentation=Allowed)
*Apr  8 15:11:55.624: //-1/xxxxxxxxxxxx/CCAPI/ccCallSetupRequest:
   Destination Pattern=00T, Called Number=00640123456789, Digit Strip=FALSE
*Apr  8 15:11:55.628: //-1/xxxxxxxxxxxx/CCAPI/ccCallSetupRequest:
   Calling Number=1212121212(TON=National, NPI=ISDN, Screening=Not Screened, Presentation=Allowed),
   Called Number=00640123456789(TON=International, NPI=ISDN),
   Redirect Number=444444, Display Info=
   Account Number=, Final Destination Flag=FALSE,
   Guid=7C2476D7-9F95-11E2-8098-B73EFBDBDE30, Outgoing Dial-peer=10
*Apr  8 15:11:55.628: //-1/xxxxxxxxxxxx/CCAPI/cc_api_display_ie_subfields:
   ccCallSetupRequest:
   cisco-username=
   ----- ccCallInfo IE subfields -----
   cisco-ani=1212121212
   cisco-anitype=2
   cisco-aniplan=1
   cisco-anipi=0
   cisco-anisi=0
   dest=00640123456789
   cisco-desttype=1
   cisco-destplan=1
   cisco-rdie=74
   cisco-rdn=444444
   cisco-rdntype=0
   cisco-rdnplan=0
   cisco-rdnpi=0
   cisco-rdnsi=0
   cisco-redirectreason=1   fwd_final_type =0
   final_redirectNumber =
   hunt_group_timeout =0

*Apr  8 15:11:55.628: //-1/xxxxxxxxxxxx/CCAPI/ccIFCallSetupRequestPrivate:
   Interface=0x65E74E90, Interface Type=6, Destination=, Mode=0x0,
   Call Params(Calling Number=1212121212,(Calling Name=1212121212)(TON=National, NPI=ISDN, Screening=Not Screened, Presentation=Allowed),
   Called Number=00640123456789(TON=International, NPI=ISDN), Calling Translated=FALSE,
   Subscriber Type Str=, FinalDestinationFlag=FALSE, Outgoing Dial-peer=10, Call Count On=FALSE,
   Source Trkgrp Route Label=, Target Trkgrp Route Label=, tg_label_flag=0, Application Call Id=)
*Apr  8 15:11:55.628: //-1/xxxxxxxxxxxx/CCAPI/cc_get_feature_vsa:
   
*Apr  8 15:11:55.628: :cc_get_feature_vsa malloc success
*Apr  8 15:11:55.628: //-1/xxxxxxxxxxxx/CCAPI/cc_get_feature_vsa:
   
*Apr  8 15:11:55.628:  cc_get_feature_vsa count is 3
*Apr  8 15:11:55.628: //-1/xxxxxxxxxxxx/CCAPI/cc_get_feature_vsa:
   
*Apr  8 15:11:55.628: :FEATURE_VSA attributes are: feature_name:0,feature_time:1709500256,feature_id:38
*Apr  8 15:11:55.628: //35/7C2476D78098/CCAPI/ccIFCallSetupRequestPrivate:
   SPI Call Setup Request Is Success; Interface Type=6, FlowMode=1
*Apr  8 15:11:55.628: //35/7C2476D78098/CCAPI/ccCallSetContext:
   Context=0x66D4B6A8
*Apr  8 15:11:55.628: //-1/xxxxxxxxxxxx/CCAPI/cc_find_feature_vsa:
   
*Apr  8 15:11:55.628:  Call Entry does not exist
*Apr  8 15:11:55.628: //-1/xxxxxxxxxxxx/CCAPI/cc_get_feature_vsa:
   
*Apr  8 15:11:55.628: :cc_get_feature_vsa malloc success
*Apr  8 15:11:55.628: //-1/xxxxxxxxxxxx/CCAPI/cc_get_feature_vsa:
   
*Apr  8 15:11:55.628:  cc_get_feature_vsa count is 4
*Apr  8 15:11:55.628: //-1/xxxxxxxxxxxx/CCAPI/cc_get_feature_vsa:
   
*Apr  8 15:11:55.632: :FEATURE_VSA attributes are: feature_name:0,feature_time:1709499824,feature_id:39
*Apr  8 15:11:55.632: //-1/xxxxxxxxxxxx/CCAPI/cc_update_feature_vsa:
   
*Apr  8 15:11:55.632:  feature_vsa is 65E4E758,featname is 0
*Apr  8 15:11:55.632: //-1/xxxxxxxxxxxx/CCAPI/cc_get_feature_vsa:
   
*Apr  8 15:11:55.632: :cc_get_feature_vsa malloc success
*Apr  8 15:11:55.632: //-1/xxxxxxxxxxxx/CCAPI/cc_get_feature_vsa:
   
*Apr  8 15:11:55.632:  cc_get_feature_vsa count is 5
*Apr  8 15:11:55.632: //-1/xxxxxxxxxxxx/CCAPI/cc_get_feature_vsa:
   
*Apr  8 15:11:55.632: :FEATURE_VSA attributes are: feature_name:0,feature_time:1709499608,feature_id:40
*Apr  8 15:11:55.632: //-1/xxxxxxxxxxxx/CCAPI/cc_update_feature_vsa:
   
*Apr  8 15:11:55.632: : Generating new featurevsa,inserting it
*Apr  8 15:11:55.632: //-1/xxxxxxxxxxxx/CCAPI/cc_update_feature_vsa:
   
*Apr  8 15:11:55.632:  feature call forward featname is 2
*Apr  8 15:11:55.632: //-1/xxxxxxxxxxxx/CCAPI/cc_free_feature_vsa:
   
*Apr  8 15:11:55.632: :cc_free_feature_vsa freeing 65E4E5A8
*Apr  8 15:11:55.632: //-1/xxxxxxxxxxxx/CCAPI/cc_free_feature_vsa:
   
*Apr  8 15:11:55.632:  vsacount in free is 4
*Apr  8 15:11:55.652: //35/7C2476D78098/CCAPI/cc_api_call_proceeding:
   Interface=0x65E74E90, Progress Indication=NULL(0)
*Apr  8 15:11:56.732: //35/7C2476D78098/CCAPI/cc_api_call_alert:
   Interface=0x65E74E90, Progress Indication=NULL(0), Signal Indication=NOT PRESENT(255)
*Apr  8 15:11:56.732: //35/7C2476D78098/CCAPI/cc_api_call_alert:
   Call Entry(Retry Count=0, Responsed=TRUE)
*Apr  8 15:11:59.284: //35/7C2476D78098/CCAPI/cc_api_call_connected:
   Interface=0x65E74E90, Data Bitmask=0x1, Progress Indication=NULL(0),
   Connection Handle=0
*Apr  8 15:11:59.284: //35/7C2476D78098/CCAPI/cc_api_call_connected:
   Call Entry(Connected=TRUE, Responsed=TRUE, Retry Count=0)
*Apr  8 15:12:10.612: //33/7C2169778094/CCAPI/cc_api_call_disconnected:
   Cause Value=18, Interface=0x65C57F24, Call Id=33
*Apr  8 15:12:10.612: //33/7C2169778094/CCAPI/cc_api_call_disconnected:
   Call Entry(Responsed=TRUE, Cause Value=18, Retry Count=0)
*Apr  8 15:12:10.612: //34/7C2169778094/CCAPI/cc_api_call_disconnected:
   Cause Value=102, Interface=0x65C57F24, Call Id=34
*Apr  8 15:12:10.612: //34/7C2169778094/CCAPI/cc_api_call_disconnected:
   Call Entry(Responsed=FALSE, Cause Value=102, Retry Count=0)
*Apr  8 15:12:10.612: //34/7C2169778094/CCAPI/ccCallDisconnect:
   Cause Value=15, Tag=0x0, Call Entry(Previous Disconnect Cause=0, Disconnect Cause=102)
*Apr  8 15:12:10.612: //34/7C2169778094/CCAPI/ccCallDisconnect:
   Cause Value=102, Call Entry(Responsed=TRUE, Cause Value=102)
*Apr  8 15:12:10.612: //34/7C2169778094/CCAPI/cc_api_get_transfer_info:
   Transfer Number Is Null
*Apr  8 15:12:10.616: //35/7C2476D78098/CCAPI/ccCallDisconnect:
   Cause Value=102, Tag=0x0, Call Entry(Previous Disconnect Cause=0, Disconnect Cause=0)
*Apr  8 15:12:10.616: //35/7C2476D78098/CCAPI/ccCallDisconnect:
   Cause Value=102, Call Entry(Responsed=TRUE, Cause Value=102)
*Apr  8 15:12:10.616: //35/7C2476D78098/CCAPI/cc_api_get_transfer_info:
   Transfer Number Is Null
*Apr  8 15:12:10.620: csim_do_test: cid(33), ev(12), disp(0)
*Apr  8 15:12:10.620: csimTraceSct: cid(33),st(0),oldst(0)
*Apr  8 15:12:10.620: csim err csimDisconnected recvd DISC cid(33) 
*Apr  8 15:12:10.620: //33/7C2169778094/CCAPI/ccCallDisconnect:
   Cause Value=18, Tag=0x0, Call Entry(Previous Disconnect Cause=0, Disconnect Cause=18)
*Apr  8 15:12:10.620: //33/7C2169778094/CCAPI/ccCallDisconnect:
   Cause Value=18, Call Entry(Responsed=TRUE, Cause Value=18)
*Apr  8 15:12:10.620: //33/7C2169778094/CCAPI/cc_api_get_transfer_info:
   Transfer Number Is Null
*Apr  8 15:12:10.620: //34/7C2169778094/CCAPI/cc_api_call_disconnect_done:
   Disposition=0, Interface=0x65C57F24, Tag=0x0, Call Id=34,
   Call Entry(Disconnect Cause=102, Voice Class Cause Code=0, Retry Count=0)
*Apr  8 15:12:10.620: //34/7C2169778094/CCAPI/cc_api_call_disconnect_done:
   Call Disconnect Event Sent
*Apr  8 15:12:10.620: //-1/xxxxxxxxxxxx/CCAPI/cc_free_feature_vsa:
   
*Apr  8 15:12:10.620: :cc_free_feature_vsa freeing 65E4E830
*Apr  8 15:12:10.620: //-1/xxxxxxxxxxxx/CCAPI/cc_free_feature_vsa:
   
*Apr  8 15:12:10.620:  vsacount in free is 3
*Apr  8 15:12:10.624: //33/7C2169778094/CCAPI/cc_api_call_disconnect_done:
   Disposition=0, Interface=0x65C57F24, Tag=0x0, Call Id=33,
   Call Entry(Disconnect Cause=18, Voice Class Cause Code=0, Retry Count=0)
*Apr  8 15:12:10.624: //33/7C2169778094/CCAPI/cc_api_call_disconnect_done:
   Call Disconnect Event Sent
*Apr  8 15:12:10.624: //-1/xxxxxxxxxxxx/CCAPI/cc_free_feature_vsa:
   
*Apr  8 15:12:10.624: :cc_free_feature_vsa freeing 65E4E680
*Apr  8 15:12:10.624: //-1/xxxxxxxxxxxx/CCAPI/cc_free_feature_vsa:
   
*Apr  8 15:12:10.624:  vsacount in free is 2
*Apr  8 15:12:10.628: csim_do_test: cid(33), ev(13), disp(0)
*Apr  8 15:12:10.628: csimTraceSct: cid(33),st(2),oldst(0)
*Apr  8 15:12:10.944: //35/7C2476D78098/CCAPI/cc_api_call_disconnect_done:
   Disposition=0, Interface=0x65E74E90, Tag=0x0, Call Id=35,
   Call Entry(Disconnect Cause=102, Voice Class Cause Code=0, Retry Count=0)
*Apr  8 15:12:10.944: //35/7C2476D78098/CCAPI/cc_api_call_disconnect_done:
   Call Disconnect Event Sent
*Apr  8 15:12:10.944: //-1/xxxxxxxxxxxx/CCAPI/cc_free_feature_vsa:
   
*Apr  8 15:12:10.944: :cc_free_feature_vsa freeing 65E4E4D0
*Apr  8 15:12:10.944: //-1/xxxxxxxxxxxx/CCAPI/cc_free_feature_vsa:
   
*Apr  8 15:12:10.944:  vsacount in free is 1
*Apr  8 15:12:10.944: //-1/xxxxxxxxxxxx/CCAPI/cc_free_feature_vsa:
   
*Apr  8 15:12:10.944:  vsacount in free is 0
*Apr  8 15:12:11.128: csim: loop = 1, failed = 1  
*Apr  8 15:12:11.128: csim: call attempted = 1, setup failed = 1, tone failed = 0

*Apr  8 15:12:11.128: //-1/xxxxxxxxxxxx/CCAPI/ccAppShutdownMode:
   ccAppShutdownMode: remove it from the queue